2027 Carpentry Project Scenario

A local customer would like a Double Chair Bench constructed for their patio (refer to the 2018 project available on la-ffa.org). The bench should meet the following specifications:
· Overall bench length must be between 68 and 72 inches, measured from the outside of one leg brace to the outside of the opposite leg brace.

· The seat height of each chair should be 15 inches from the ground.
· The armrests should be positioned 24 inches from the ground.
· The center table should measure 18 inches wide by 23¾ inches long, with the tabletop aligned to the same height as the armrests (24 inches from the ground).

· The customer would like two recessed 4” diameter cup holders incorporated into the center tabletop and positioned toward the front of the table for easy access.

· The tops of the chair backs should feature a rounded design rather than a square profile.
The completed project should be sturdy, functional, and aesthetically pleasing while meeting all specified dimensions and customer preferences.
____________________________________________________________________________________
Information needed in the Blueprint for the Double Chair Bench
The Blueprint should be organized accordingly: 
Page 1 - One cover page to include a materials list and cut list (Typed)
Page 2 - One page with a drawing of the front view 
Page 3 - One page with drawings of the side view
Page 4 - One page with a drawing of a top view 
Page 5 - One page with a drawing of the rear view (Special View)
Page 6 - One page with a drawing of the cupholder assembly (Special View)

*You may have more pages than this, but this is the minimum requirement. 
Use this link to access the example blueprint to note what information your teams should include when drafting each view of the project. Carpentry : Career and Leadership Development Events : Portal : Louisiana FFA
